QualSoft Software Consultants
http://www.qualsoftsoftware.com
30/10/2002

QUALSOFT MAKES NO WARRANTIES, EITHER
EXPRESS OR IMPLIED, REGARDING THE ENCLOSED SOFTWARE, INCLUDING
MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.  

QUALSOFT EXCLUDES ANY WARRANTY COVERAGE FOR INCIDENTAL OR 
CONSEQUENTIAL DAMAGES.  

Windows NT Printer Driver for Godex EZ thermal product.

Setting up the Driver
---------------------

To install the driver perform the following steps:

Windows NT 
----------

- Boot into Windows NT,
- select Start,
- select Settings, 
- select Printers, Add printer and continue to 'Have Disk'.
- select drive e.g. A:\
- You will then be presented with the supported Godex EZ thermal models,
- Double click on the required printer driver.
- The Driver will now install.


Removal/upgrading of the Driver
---------------------
It is essential that the following steps are followed when upgrading the 
driver.

- select Start, Settings, Printers and delete any previously installed Godex 
  EZ thermal drivers, 
- Perform a RESTART and Boot into Windows NT,
- select Start,
- select Settings, 
- select Printers, Add printer and continue to 'Have Disk'.
- select drive e.g. A:\
- You will then be presented with the supported Godex thermal models,
- Double click on the required printer driver.
- The Driver will now install.

NOTE: For your information the following files are installed in the 
        winnt\system32\spool\drivers\w32x86 directory.

        - GDXEZNT.DLL
        - GDXMSGE.DLL
        - GODEXUI.DLL
        - GDXBMPS.DLL
        - DLSBAR32.DLL
        Note: These files will be located in directories w32x86, 
              or w32x86/1 or /2

To remove the installed barcode display font perform the following:
        - close the Command Prompt Window.
        - Select Start->Settings->Control Panel and select Fonts
        - Delete the following fonts:
                - QSBar

If any problems are found please notify your nearest Godex dealer, 
in order to rectify any problems should they exist.

Application Notes.
-----------------

Accessing COM ports from DOS.
-----------------------------
Installation of printer drivers and using them in conjunction with serial 
communication locks access to the COM port when using DOS software from 
within a DOS prompt. 
